**Care and Maintenance Sheet**

March 2020

**Stone:** Bluestone

NB: These are general recommendations only, for technical advice please don’t hesitation to call iRock Finishes - **1300 131 271**

*Bluestone Recommended Care and Maintenance*

**Daily/Weekly:**

1. Mop up spills as soon as possible, using a pH neutral cleaner.
2. For general cleaning, mop over all surfaces using a pH neutral cleaner at a ratio 1:100 with warm or cold water.
3. For problem spots:
   1. use a doodle bug fitted with a blue pad and a pH neutral cleaner on the problem area
   2. mop the area with a damp mop.
4. Please have us advise on heavy spills (oils, acidic, salts, etc.), although most can be corrected with similar methods as above, using appropriate cleaners and/or diamond polishing pads.

**6-12 Months:**

1. Slowly pass over entire surface with an auto scrubber and/or pressure washer with a pH Neutral cleaner. Remove excess water with a wet vacuum and mop according to instructions above.
2. For edges:
   1. use a doodle bug fitted with a blue pad and pH neutral cleaner
   2. mop over edges with a damp mop.

**3-5 Years:**

1. Consider resealing your bluestone.

.